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B: distance to water line
D extemal flange diameter
£ intemal lange diameter
F bolt holes diameter

6 bolt position radius from the centre.
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